DallFlex 2.0: The original is now even better

Arnsberg, March 2025

Press release

Proven shower channel system with new features

Arnsberg-based drainage specialist Dallmer always designs its solutions in close dialog with installers, planners and architects. The best example of this is DallFlex 2.0, the enhanced drainage system with new features.

Why a further development?

DallFlex is an established system for level-access showers that impresses with its flexibility and ease of installation. However, the requirements of the industry are constantly evolving - and Dallmer is developing with them. In intensive discussions with fabricators, the family-owned company has identified potential for optimization in order to make handling even easier and more efficient. True to the motto: Together we make drainage simple.

Future-proof solution for thinner coverings

The construction industry is increasingly focusing on thinner coverings from 6 mm. Whether thin-layered trowel floors, ceramic tiles or natural stone: the DallFlex 2.0 drainage system offers maximum design freedom for floor-level showers and enables the installation of very thin materials from 6 mm. And what's special: This applies to the entire DallFlex portfolio with more than 10 shower channels. Architects, planners and installers benefit equally from the new flexibility and installation reliability.

Sophisticated features for even more comfort

The enhanced generation includes the following new features, among others:

* Efficient installation thanks to factory pre-assembled mounting unit with integrated positioning aid:

The integrated positioning aid ensures precise alignment with wall and floor coverings. In addition, the 180-degree rotatable frame offers maximum design freedom thanks to the variable choice of covering thicknesses.

* Quick-release system for easy height adjustment:

The quick-release system enables effortless presetting and precise height adjustment of the fixable threaded rod. The sound-decoupled mounting feet can be conveniently adjusted.

* Innovative mechanical odor trap:

Already familiar from the tried-and-tested DallDrain system: the mechanical odor trap with magnetic closing mechanism permanently prevents unpleasant drain gases - without the need for sealing water. A clear advantage for both the mechanical and water-guided odor trap: cleaning and maintenance are quick and easy at any time.

In addition, the clear interface between tiler and installer has been strengthened by reducing the number of individual parts.

Proven advantages remain

In addition to the new features, the familiar strengths of the DallFlex system remain: The flexible, crease-free and click-in sealing sleeve ensures a secure connection to composite seals in accordance with DIN 18534. The drain support with ball joint, which can be positioned on three sides without tools, ensures a stress-free connection to the waste water pipe.

With DallFlex 2.0, Dallmer offers an even more sophisticated, future-proof drainage solution that makes everyday work easier for installers and opens up new design options for architects and planners in combination with the designer shower channel range.

Further information:

dallmer.com